	Weights

	Take off weight
	3000

	Maximum take off
	3300

	Maximum useful load
	1300

	Powerplant

	Type
	PW207K x 2

	Take off power
	630 shp

	Maximum continious power
	561 shp

	*ratings per engine, standard day, sea level

	Performance

	VNE
	285 km/h

	Cruise speed
	250 km/h

	Maximum rate of climb
	21,5 m/c

	Service ceiling
	5700 m

	Hover ceiling OGE
	3300 m

	Maximum range
	635 km

	Dimensions

	Overall length
	13.543 m

	Overall height
	3.56 m

	Fuselage length, without tail boom
	6.910 m

	Main gear tread
	2.50 m

	Cabin length
	4.60 m

	Cabin width
	1.68 m

	Cabin height
	1.3 m

	Capacity
	9 + 1 pilot


